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Features	
· High quality image with 8 MP, 1/2.7" CMOS sensor
· 8 MP (3840 × 2160)@20 fps; 5 MP (3072 × 1728)@30/25 fps; 4 MP (2560 × 1440)@30/25 fps; 1080P (1920 × 1080)@30/25 fps
· Ultra 265, H.265, H.264, MJPEG
· 120 dB true WDR technology enables clear image in strong light scene
· Supports 9:16 corridor mode
· Built‑in mic
· Smart IR, up to 30 m (98.4 ft.) IR distance
· MicroSD, up to 512 GB
· IP67 protection
· Supports PoE power supply
· 3‑axis
Specifications	
	Model
	E1T-8F28-DL

	Camera

	Max Resolution
	8 MP

	Sensor
	1/2.7" CMOS

	Min. Illumination
	Color: 0.005 Lux (F1.6, AGC ON), 0 Lux with light

	Day/Night
	IR‑cut filter with auto switch (ICR)

	Shutter
	Auto/Manual, 1 ~ 1/100000s

	Adjustment Angle
	Pan: 0° to 360°, Tilt: 0° to 80°, Rotate: 0° to 360°

	S/N
	>56 dB

	WDR
	120 dB

	Lens

	Focal Length
	2.8 mm

	Iris Type
	Fixed

	Iris
	F1.6

	Field of View (H)
	100.8°

	Field of View (V)
	55.8 °

	Field of View (D)
	105.7°

	Lens Type
	Fixed

	DORI

	DORI Distance (Lens)
	2.8 mm

	DORI Distance (Detect)
	84.0 m (275.6 ft.)

	DORI Distance (Observe)
	33.6 m (110.2 ft.)

	DORI Distance (Recognize)
	16.8 m (55.1 ft.)

	DORI Distance (Identify)
	8.4 m (27.6 ft.)

	Illuminator

	Supplemental Light
	Dual light

	Illumination Distance (IR)
	30 m (98.4 ft.)

	Illumination Distance (Warm Light)
	30 m (98.4 ft.)

	Wavelength
	850 nm

	Light On/Off Control
	Auto/Manual

	Video

	Video Compression
	Ultra 265, H.265, H.264, MJPEG

	H.264 Code Profile
	Baseline profile, Main profile, High profile

	Frame Rate
	Main Stream: 8 MP (3840 × 2160), max. 20 fps; 5 MP (3072 × 1728), max. 30 fps; 4 MP (2560 × 1440), max. 30 fps; 1080P (1920 × 1080), max. 30 fps; 720P (1280 × 720), max. 30 fps;
Sub Stream: 1080P (1920 × 1080), max. 30 fps; 720P (1280 × 720), max. 30 fps; D1 (720 × 576), max. 30 fps; 640 × 360, max. 30 fps; 2CIF (704 × 288), max. 30 fps; CIF (352 × 288), max. 30 fps;

	Video Bit Rate
	128 Kbps to 16 Mbps

	U‑code
	Support

	OSD
	Up to 4 OSDs

	Privacy Mask
	Up to 4 areas

	ROI
	Support

	Video Stream
	Dual streams

	Image

	White Balance
	Auto, Outdoor, Fine tune, Sodium lamp, Locked, Auto2, Area white balance

	Digital Noise Reduction
	2D/3D DNR

	Smart IR
	Support

	Flip
	Normal, Flip vertical, Flip horizontal, 180°, 90° Clockwise, 90° Anti‑clockwise

	Dewarping
	N/A

	HLC
	Support

	BLC
	Support

	Defog
	Digital defog

	Image Stabilization
	N/A

	Events

	Basic Detection
	Motion detection, Tampering alarm, Audio detection, Human body detection

	General Function
	Watermark, IP address filtering, Access policy, ARP protection, RTSP authentication, User authentication, HTTP authentication

	Audio

	Audio Compression
	G.711U, G.711A

	Audio Bitrate
	64 Kbps

	Two‑way Audio
	N/A

	Suppression
	Support

	Sampling Rate
	8 kHz

	Storage

	Edge Storage
	MicroSD, up to 512 GB

	Network Storage
	ANR, NAS (NFS)

	Network

	Protocols
	IPv4, IGMP, ICMP, ARP, TCP, UDP, DHCP, RTP, RTSP, RTCP, RTMP, DNS, DDNS, NTP, FTP, UPnP, HTTP, HTTPS, SMTP, SSL/TLS, SNMP, QoS, 802.1x

	Compatible Integration
	ONVIF (Profile S, Profile G, Profile T), API, SDK

	User/Host
	Up to 32 users. 3 user levels: administrator, common user and operator

	Security
	Password Protection, Strong Password, HTTPS Encryption, Export Operation Logs, Basic and Digest Authentication for RTSP, Digest Authentication for HTTP, TLS 1.2, WSSE and Digest Authentication for ONVIF

	Client
	UNV‑Link, UNV‑Link Pro, EZStation

	Web Browser
	Plug‑in required live view: IE 10+, Chrome 45+, Firefox 52+, Edge 79+, Plug‑in free live view: Chrome 57+, Firefox 58+, Edge 16+

	Interface

	Audio I/O
	N/A

	Alarm I/O
	N/A

	Serial Port
	N/A

	Built‑in Mic
	Support

	Built‑in Speaker
	N/A

	WIFI
	N/A

	Network
	1 × RJ45 10 M/100 M Base‑TX Ethernet

	Video Output
	N/A

	Certification

	EMC
	CE‑EMC (EN 55032, EN 61000‑3‑3, EN IEC 61000‑3‑2, EN 50130‑4)
FCC (FCC 47 CFR part15 B)

	Safety
	CE LVD (EN 62368‑1)
UL/CUL (UL 62368‑1, CAN/CSA C22.2 No. 62368‑1)

	Environment
	CE‑RoHS (2011/65/EU;(EU)2015/863)
WEEE (2012/19/EU)
Packaging and Packaging Waste (94/62/EC)

	Protection
	IP67 (IEC 60529)

	General

	Power Consumption
	Max. 5.3 W

	Power
	DC 12 V±25%, PoE (IEEE 802.3af)

	Weight
	0.29 kg (0.64 lb.)

	Power Interface
	Ø5.5 mm coaxial power plug

	Dimensions
	Ø126 mm × 93.6 mm (Ø5.0" × 3.7") (Ø × H)

	Material
	Metal + Plastic

	Working Environment
	‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Storage Environment
	‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Surge Protection
	4 KV

	Reset Button
	N/A

	Web Client Language
	13 Languages: English, Simplified Chinese, Polish, German, Russian, French, Korean, Dutch, Czech, Portuguese, Spanish, Spanish (Europe), Italian


Dimensions	
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Accessories	
	TR-JB03-H-IN-V2
	TR-JB03-H-IN
	TR-JB07/WM03-F-IN-V2

	Junction Box for Metal Turret Camera(Support wiring from behind)
	Junction Box for Metal Turret Camera(Support wiring from behind)
	Wall Mounting Assembling Bracket with Back Hole for 3 Inch Hemisphere
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	TR-WM03-B-IN-V2
	TR-UP06-C-IN-V2
	TR-A01-IN

	Wall Mounting Assembling Bracket for 3 Inch Hemisphere
	Pole Mounting Bracket for Bullet Junction Box Only
	NPT 3/4'' Waterproof Cable Gland
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	TR-SE24-IN
	TR-SE24-A-IN
	TR-CM24-IN

	Dome Pendent Mounting Pole 200mm
	Dome Pendent Mounting Pole 500mm
	Dome Pendent Mounting Bracket(Indoor)
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	TR-WM03-B-IN
	TR-JB07/WM03-F-IN
	TR-UC08-C

	Wall Mounting Assembling Bracket for 3 Inch Hemisphere
	Wall Mounting Assembling Bracket with Back Hole for 3 Inch Hemisphere
	Bullet&Dome Corner Mounting Bracket
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	TR-UC08-C-V2
	
	

	Bullet&Dome Corner Mounting Bracket
	
	

	[image: C:\Users\x04297\Desktop\渲染图\TR-JB05-B-IN\TR-JB05-B-IN-1.png]
	
	




1
2

2
	
image4.png




image5.png
4K




image6.png
4 A

Gl

ColorHunter

\ 4




image7.png




image8.png
4 A

e
| smartir

e
L 4




image9.png
Edga storage

L 4




image10.png
PoE




image11.png
i
1P§7




image12.png
NDAA

COMPLIANT

NDAA Compliant




image13.png




image14.png




image15.png




image16.png




image17.png




image18.png




image19.png




image20.png




image21.png




image22.png




image23.png




image24.png
e





image3.png




image25.png
Y




image26.png




