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Features	
· High quality image with 4 MP, 1/1.8" CMOS sensor and F1.0 large aperture lens
· 4 MP (2688 × 1520)@25/20 fps; 4 MP (2560 × 1440)@25/20 fps; 3 MP (2304 × 1296)@30/25 fps; 1080P (1920 × 1080)@30/25 fps
· Ultra 265, H.265, H.264, MJPEG(Sub Stream Only)
· Supports Wise‑ISP technology, deeply optimizing color, detail, and smear effects in extremely low‑light scenes
· Support cross line, intrusion detection (based on human body detection and vehicle detection)
· Support ultra motion detection (human/ vehicle detection)
· 120 dB true WDR technology enables clear image in strong light scene
· Supports 9:16 corridor mode
· Built‑in mic
· White light, up to 30 m (98.4 ft) warm light distance
· MicroSD, up to 512 GB
· IP67 protection
· Supports PoE power supply
Specifications	
	Model
	O1T-4F28

	Camera

	Max Resolution
	4 MP

	Sensor
	1/1.8" CMOS

	Min. Illumination
	Color: 0.0003 Lux (F1.0, AGC ON)

	Shutter
	Auto/Manual, 1 to 1/100000 s

	Adjustment Angle
	Pan: 0° to 360°, Tilt: 0° to 75°, Rotate: 0° to 360°

	S/N
	> 52 dB

	WDR
	120 dB

	Lens

	Focal Length
	2.8 mm

	Iris
	F1.0

	Field of View (H)
	117.7 °

	Field of View (V)
	68.7 °

	Field of View (D)
	140.7 °

	Lens Type
	Fixed

	Iris Type
	Fixed

	DORI

	DORI Distance (Lens)
	2.8 mm

	DORI Distance (Detect)
	61.4 m (201.5 ft)

	DORI Distance (Observe)
	24.6 m (80.6 ft)

	DORI Distance (Recognize)
	12.3 m (40.3 ft)

	DORI Distance (Identify)
	6.1 m (20.2 ft)

	Illuminator

	Illumination Distance (Warm Light)
	30 m (98.4 ft)

	Light On/Off Control
	Auto/Manual

	Supplemental Light
	Warm light

	Video

	Video Compression
	Ultra 265, H.265, H.264, MJPEG (Sub Stream Only)

	H.264 Code Profile
	Baseline profile, Main profile, High profile

	Frame Rate
	Main Stream: 4 MP (2688 × 1520), max. 25 fps; 4 MP (2560 × 1440), max. 25 fps; 3 MP (2304 × 1296), max. 30 fps; 1080P (1920 × 1080), max. 30 fps;720P (1280 × 720), max. 30 fps；
Sub Stream: 720P (1280 × 720), max. 30 fps; D1 (720 × 576), max. 30 fps; 640 × 360, max. 30 fps; 2CIF (704 × 288), max. 30 fps; CIF (352 × 288), max. 30 fps

	Video Bit Rate
	128 Kbps to 6144 Kbps

	OSD
	Up to 4 OSDs

	Privacy Mask
	Up to 4 areas

	ROI
	Up to 8 areas

	U‑code
	Support

	Video Stream
	Dual streams

	Snapshot
	Support

	Snapshot Resolution
	2688*1520; 2560 × 1440; 2304 × 1296; 1920 × 1080; 1280 × 720; 720 × 576; 640 × 360; 704 × 288; 352 × 288

	Image

	Smart Illumination
	Support

	White Balance
	Auto, Outdoor, Fine tune, Sodium lamp, Locked, Auto2, Area white balance

	Digital Noise Reduction
	2D/3D DNR

	Flip
	Normal, Flip vertical, Flip horizontal, 180°, 90° Clockwise, 90° Anti‑clockwise

	HLC
	Support

	Dewarping
	N/A

	BLC
	Support

	Defog
	Digital defog

	Intelligent

	Smart Intrusion Prevention (Lite)
	Intrusion, crossline detection (both detection are based on human body and vehicle detection)

	Events

	Basic Detection
	Motion detection, Ultra motion detection (based on human body and vehicle detection), Tampering alarm, Audio detection

	General Function
	Watermark, IP address filtering, Access policy, ARP protection, RTSP authentication, User authentication, HTTP authentication

	Audio

	Audio Compression
	G.711U, G.711A, AAC‑LC

	Audio Bitrate
	G.711U/G.711A: 64 kbps, AAC‑LC: 128 kbps

	Two‑way Audio
	N/A

	Suppression
	Support

	Sampling Rate
	G.711U/G.711A: 8 kHz, AAC‑LC: 8 kHz, 16 kHz, 48 kHz

	Storage

	Edge Storage
	MicroSD, up to 512 GB

	Network Storage
	ANR, NAS (NFS)

	Network

	Protocols
	IPv4, IPv6, IGMP, ICMP, ARP, TCP, UDP, DHCP, PPPoE, RTP, RTSP, RTCP, DNS, DDNS, NTP, FTP, UPnP, HTTP, HTTPS, SMTP, 802.1x, SNMP, QoS, RTMP, SSL/TLS

	Compatible Integration
	ONVIF (Profile S, Profile G, Profile T), API, SDK

	Client
	EZStation, APP

	Web Browser
	Plug‑in required live view: IE 10+, Chrome 45+, Firefox 52+, Edge 79+, Plug‑in free live view: Chrome 57+, Firefox 58+, Edge 16+

	Security
	Password protection, Strong Password, HTTPS encryption, Export operation logs, Basic and Digest Authentication for RTSP, Digest Authentication for HTTP, TLS 1.2, WSSE and Digest Authentication for ONVIF

	User/Host
	Up to 32 users. 2 user levels: administrator and common user

	Interface

	Audio I/O
	N/A

	Alarm I/O
	N/A

	Serial Port
	N/A

	Built‑in Mic
	Support

	Built‑in Speaker
	N/A

	WIFI
	N/A

	Network
	1 × RJ45 10 M/100 M Base‑TX Ethernet

	Video Output
	N/A

	Certification

	EMC
	CE‑EMC (EN 55032, EN 61000‑3‑3, EN IEC 61000‑3‑2, EN 50130‑4)
FCC (FCC 47 CFR part15 B)

	Safety
	CE‑LVD (EN 62368‑1)
UL/CUL (UL 62368‑1, CAN/CSA C22.2 No. 62368‑1)

	Environment
	CE‑RoHS (2011/65/EU ; (EU) 2015/863) ; WEEE (2012/19/EU)

	Protection
	IP67 (IEC 60529)

	General

	Power
	DC 12 V±25%, PoE (IEEE 802.3af)

	Power Consumption
	Max. 3 W

	Power Interface
	Ø5.5 mm coaxial power plug

	Dimensions
	Ø118 mm × 108 mm (Ø4.6" × 4.3") (Ø × H)

	Material
	Metal

	Working Environment
	‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Storage Environment
	‑30 ℃ to 60 ℃ (‑22 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Surge Protection
	4 KV

	Reset Button
	Support

	Web Client Language
	14 Languages: English, Simplified Chinese, Polish, German, Russian, French, Korean, Dutch, Czech, Portuguese, Spanish, Spanish (Europe), Italian, Turkish


Dimensions	
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Accessories	
	TR-JB03-I-IN
	TR-CM24-IN
	TR-SE24-A-IN

	Junction Box for Turret Camera(Support wiring from behind)
	Dome Pendent Mounting Bracket(Indoor)
	Dome Pendent Mounting Pole 500mm
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	TR-SE24-IN
	TR-A01-IN
	TR-JB07/WM03-G-IN-V2

	Dome Pendent Mounting Pole 200mm
	NPT 3/4'' Waterproof Cable Gland
	Wall Mounting Assembling Bracket For 32 Fix‑dome&Mini Fix‑dome&Plastic Turret Camera
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	TR-WM03-D-IN-V2
	TR-UC08-C-V2
	TR-UP06-C-IN-V2

	Wall Mounting Bracket for 32 Fix‑dome&Mini Fix‑dome&Plastic Turret Camera
	Bullet&Dome Corner Mounting Bracket
	Pole Mounting Bracket for Bullet Junction Box Only
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