[image: 背景图案

AI 生成的内容可能不正确。]		[image: 背景图案

AI 生成的内容可能不正确。]	
[image: ]产品彩页


[image: 背景图案

AI 生成的内容可能不正确。]O2T-4F28

4MP ColorHunter with Wise‑ISP Fixed Warm Light Turret Network Camera
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Features	
· High quality image with 4 MP, 1/1.8" CMOS sensor
· 4 MP (2688 × 1520)@30/25 (default) fps; 4 MP (2560 × 1440)@30/25 fps; 3 MP (2304 × 1296)@30/25 fps; 1080P (1920 × 1080)@30/25 fps
· Ultra 265, H.265, H.264, MJPEG
· ColorHunter with Wise‑ISP technology ensures 24‑hour full‑color images
· Intelligent perimeter protection, including cross line, intrusion, enter area, leave area detection
· Based on target classification, smart intrusion prevention significantly reduces false alarm caused by leaves, birds and lights, accurately focusing on human, motor vehicle and non‑motor vehicle
· Intelligent people flow counting and crowd density monitoring
· Smart intrusion prevention with color retrieval
· ASM (auto scene match)
· 130 dB true WDR technology enables clear image in strong light scene
· Supports 9:16 corridor mode
· Alarm I/O: 1/1, audio I/O: 1/1, built‑in mic
· White light, up to 30 m (98.4 ft) warm light distance
· MicroSD, up to 512 GB
· Supports NEMA 4X, IK10 vandal resistant and IP67 protection
Specifications	
	Model
	O2T-4F28

	Camera

	Max Resolution
	4 MP

	Sensor
	1/1.8" CMOS

	Min. Illumination
	Color: 0.0003 Lux (F1.0, AGC ON)

	Shutter
	Auto/Manual, 1 to 1/100000 s

	Adjustment Angle
	Pan: 0° to 360°, Tilt: 0° to 75°, Rotate: 0° to 360°

	S/N
	>56 dB

	WDR
	130 dB

	Lens

	Focal Length
	2.8 mm

	Iris Type
	Fixed

	Iris
	F1.0

	Field of View (H)
	110.4°

	Field of View (V)
	60.5°

	Field of View (D)
	115.2°

	Lens Type
	Fixed

	DORI

	DORI Distance (Lens)
	2.8 mm

	DORI Distance (Detect)
	43.4 m (142.4 ft)

	DORI Distance (Observe)
	17.4 m (57.1 ft)

	DORI Distance (Recognize)
	8.7 m (28.5 ft)

	DORI Distance (Identify)
	4.3 m (14.1 ft)

	Illuminator

	Supplemental Light
	Warm light

	Illumination Distance (Warm Light)
	30 m (98.4 ft)

	Light On/Off Control
	Auto/Manual

	Video

	Video Compression
	Ultra 265, H.265, H.264, MJPEG

	H.264 Code Profile
	Baseline profile, Main profile, High profile

	Frame Rate‑Main Stream
	4 MP (2688 × 1520), max. 30 fps; 4 MP (2560 × 1440), max. 30 fps; 3 MP (2304 × 1296), max. 30 fps; 1080P (1920 × 1080), max. 30 fps; 720P (1280 × 720), max. 30 fps

	Frame Rate‑Sub Stream
	1080P (1920 × 1080), max. 30 fps; 720P (1280 × 720), max. 30 fps; D1 (720 × 576), max. 30 fps; 640 × 360, max. 30 fps; 2CIF (704 × 288), max. 30 fps; CIF (352 × 288), max. 30 fps

	Frame Rate‑Third Stream
	D1 (720 × 576), max. 30 fps; 640 × 360, max. 30 fps; 2CIF (704 × 288), max. 30 fps; CIF (352 × 288), max. 30 fps

	Video Bit Rate
	128 Kbps to 16 Mbps

	U‑code
	Support

	OSD
	Up to 8 OSDs

	Privacy Mask
	Up to 4 areas

	ROI
	Support

	Video Stream
	Triple streams

	Image

	White Balance
	Auto, Outdoor, Fine tune, Sodium lamp, Locked, Auto2

	Digital Noise Reduction
	2D/3D DNR

	Flip
	Normal, Flip vertical, Flip horizontal, 180°, 90° Clockwise, 90° Anti‑clockwise

	Dewarping
	N/A

	HLC
	Support

	BLC
	Support

	Defog
	Digital defog

	Intelligent

	Statistical Analysis
	N/A

	People Counting
	Support people flow counting and crowd density detection

	Attribute Collection
	SIP with color retrieval

	Events

	Basic Detection
	Motion detection, Ultra motion detection, Tampering alarm, Audio detection, Object removed, Object Left Behind

	General Function
	Watermark, IP address filtering, Access policy, ARP protection, RTSP authentication, User authentication, HTTP authentication, Alarm input, Alarm output

	Audio

	Audio Compression
	G.711U, G.711A, AAC‑LC

	Audio Bitrate
	G.711U/G.711A: 64 kbps, AAC‑LC: 128 kbps

	Two‑way Audio
	Support

	Suppression
	Support

	Sampling Rate
	G.711U/G.711A: 8 kHz, AAC‑LC: 8 kHz, 16 kHz, 48 kHz

	Storage

	Edge Storage
	MicroSD, up to 512 GB

	Network Storage
	ANR, NAS (NFS)

	Network

	Security
	Password Protection, Strong Password, HTTPS Encryption, Export Operation Logs, Basic and Digest Authentication for RTSP, Digest Authentication for HTTP, TLS 1.2, WSSE and Digest Authentication for ONVIF

	Protocols
	IPv4, IPv6, IGMP, ICMP, ARP, TCP, UDP, DHCP, PPPoE, RTP, RTSP, RTCP, RTMP, DNS, DDNS, NTP, FTP, UPnP, HTTP, HTTPS, SMTP, 802.1x, SNMP, QoS, SSL/TLS, SSH

	Compatible Integration
	ONVIF (Profile S, Profile G, Profile T, Profile M), API, SDK

	User/Host
	Up to 32 users. 3 user levels: administrator, common user and operator

	Client
	EZStation, APP

	Web Browser
	Plug‑in required live view: IE 10+, Chrome 45+, Firefox 52+, Edge 79+, Plug‑in free live view: Chrome 57+, Firefox 58+, Edge 16+

	Interface

	Audio I/O
	1 Input: impedance 35 kΩ, amplitude 2 V [p‑p], 1 Output: impedance 600 Ω, amplitude 2 V [p‑p]

	Alarm I/O
	1/1

	Serial Port
	N/A

	Built‑in Mic
	Support

	Built‑in Speaker
	N/A

	WIFI
	N/A

	Network
	1 × RJ45 10 M/100 M Base‑TX Ethernet

	Video Output
	N/A

	Certification

	EMC
	CE‑EMC (EN 55032, EN 61000‑3‑3, EN IEC 61000‑3‑2, EN 50130)
FCC (FCC 47 CFR part15 B)

	Safety
	CE‑LVD (EN 62368‑1)
CB (IEC 62368‑1)
UL/CUL (UL 62368‑1, CAN/CSA C22.2 No. 62368‑1)

	Environment
	CE‑RoHS (2011/65/EU;(EU)2015/863); WEEE (2012/19/EU)

	Protection
	IP67 (IEC 60529)
IK10 (IEC 62262)
NEMA 4X

	General

	Power
	DC 12 V±25%, PoE (IEEE 802.3af)

	Power Consumption
	Max. 4.5 W

	Power Interface
	Ø5.5 mm coaxial power plug

	Dimensions
	Ø129 mm × 110 mm (Ø5.1" × 4.3") (Ø × H)

	Weight
	0.67 kg (1.48 lb)

	Material
	Metal

	Working Environment
	‑40 ℃ to 60 ℃ (‑40 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Storage Environment
	‑40 ℃ to 60 ℃ (‑40 ℉ to 140 ℉), Humidity: ≤ 95% RH (non‑condensing)

	Surge Protection
	4 KV

	Reset Button
	Support

	Web Client Language
	20 Languages: Traditional Chinese, English, Simplified Chinese, Polish, German, Russian, French, Korean, Dutch, Czech, Portuguese (Europe), Portuguese (Brazil), Japanese, Thai, Turkish, Spanish (Latin America), Spanish (Europe), Hungarian, Italian, Vietnamese

	Built‑in DC12V Output
	Support


Dimensions	
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Accessories	
	TR-JB03-H-IN-V2
	TR-A01-IN
	TR-SE24-IN

	Turret Junction Box(Support Wiring From Behind)
	NPT 3/4'' Waterproof Cable Gland
	Dome Pendent Mounting Pole 200mm
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	TR-SE24-A-IN
	TR-CM24-IN
	TR-UC08-C-V2

	Dome Pendent Mounting Pole 500mm
	Dome Pendent Mounting Bracket(Indoor)
	Bullet&Dome Corner Mounting Bracket
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	TR-JB07/WM03-F-IN-V2
	TR-WM03-B-IN-V2
	TR-JB03-J-IN

	Wall Mounting Assembling Bracket with Back Hole For 3 Inches Dome
	3 Inches Dome Wall Mounting Assembling Bracket
	VF Turret Junction Box(Support Wiring From Behind)
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	TR-UP06-C-IN-V2
	
	

	Pole Mounting Bracket For Bullet Junction Box Only
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